AMD AHCI controller driver distribution list
Version 1.2.001.0275, 11/11/2010 

WS03x64	- Windows Server 2003 SP2, x64
WS03x86	- Windows Server 2003 SP2, x86
LHx64 	- Windows Server 2008, x64
LHx86 	- Windows Server 2008, x86
Win7x64	- Windows Server 2008R2, x64

Supported chipsets

SB700 family
SB800 family
Hudson-1/2/3 family

Installation Notes

You can install/uninstall the driver by running the CIM installer. This method will correctly show the driver as WHQL certified in the Device Manager.

Revision History

1.2.001.0275

-	Memory usage optimization 
-	ZPODD power on incurred 10 sec delay workaround
-	Potential DMA overrun bug fix

1.2.1.263
	
-	Performance optimization
-	Boot Optimization
-	TRIM implementation

1.2.1.238

	Renamed
-	amdsata.inf -> amd_sata.inf
-	amdsata.cat -> amd_sata.cat
-	amdsata.sys -> amd_sata.sys
-	amdxata.sys -> amd_xata.sys

Added
-	Zero Power ODD support (if enabled in BIOS; Windows 7 only); the ZPODD is powered off after 60 Sec w/o media inside and tray closed (for tray type ZPODDs)
-	DAPS support
-	DIPM Setting Index 3 added to AHCI Link Power Management Settings (in addition to existing Active(0), HIPM(1) and HIPM+DIPM(2) ) and can be chosen to any Power Scheme using the inbox utility powercfg.exe

1.2.0.197
-	Robustness improvement during hibernation / de-hibernation

1.2.0.164 

-	Minor bug fix

1.2.0.147 

-	Slight performance improvement
-	FUA is changed to be disabled by default

1.2.0.144 

-	Slight performance improvement
-	Port Multiplier enumeration optimization
-	Velocity test numbers improved

1.2.0.125 – first release